
How to add a new thunk table for a new 16-bit thunk DLL:

 - modify wow16\kernel31\kernel.def and add an export similar to __MOD_KERNEL
   rebuild the 16-bit libraries  (nmake in mvdm\wow16\lib)

 - modify the Thunk macro in inc\wow.h and add another externA
   update the MOD_ constants in wow.h, the profiling code still uses them.
   regenerate wow.inc

 - update kernel31\kdata.asm and add another MOD_ variable

 - declare and make public a new __MOD_ value for exporting  (ldboot.asm)

 - create the table (.h file) for inclusion into wowtbl.c

 - wowtbl.h  - add a field to the tableoffsets structure

 - wowtbl.c  - #include the table into aw32WOW and update apszModNames,
    InitThunkTableOffsets, ModFromCallID, and TableOffsetFromName

 - update makefile.inc with the new dependency
